|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Willow Theatre Lighting Worksheet** | | |  |  |  |  |
| **CHANNEL** | **ADDRESS** | **FIXTURE TYPE** | **LOCATION** | **FOCUS** | **COLOR** | **NOTE** |
| 1 | 1 | Dimmer | Spot Rail |  |  |  |
| 2 | 2 | Dimmer | Spot Rail |  |  |  |
| 3 | 3 | Dimmer | Spot Rail |  |  |  |
| 4 | 4 | Dimmer | Spot Rail |  |  |  |
| 5 | 5 | Source Four Ellipsoidal 26' | Catwalk | FOH USR X | NC |  |
| 6 | 6 | Source Four Ellipsoidal 26' | Catwalk | FOH USL | R60 |  |
| 7 | 7 | Source Four Ellipsoidal 26' | Catwalk | FOH USL | R5 |  |
| 8 | 8 | Source Four Ellipsoidal 26' | Catwalk | FOH DSR | R60 |  |
| 9 | 9 | Source Four Ellipsoidal 26' | Catwalk | FOH DSR | R5 |  |
| 10 | 10 | Source Four Ellipsoidal 26' | Catwalk | FOH CSR | R51 |  |
| 11 | 11 | Source Four Ellipsoidal 19' | Catwalk | FOH CSR | NC |  |
| 12 | 12 | Source Four Ellipsoidal 19' | Catwalk | FOH CS | NC |  |
| 13 | 13 | Source Four Ellipsoidal 26' | Catwalk | FOH USL | R60 |  |
| 14 | 14 | Source Four Ellipsoidal 26' | Catwalk | FOH DSC | R5 |  |
| 15 | 15 | Source Four Ellipsoidal 19' | Catwalk | FOH USC | R5 |  |
| 16 | 16 | Source Four Ellipsoidal 19' | Catwalk | FOH CSL | NC |  |
| 17 | 17 | Source Four Ellipsoidal 26' | Catwalk | FOH DSC | R60 |  |
| 18 | 18 | Source Four Ellipsoidal 26' | Catwalk | FOH CSL | R51 |  |
| 19 | 19 | Dimmer | Catwalk | EMPTY |  |  |
| 20 | 20 | Source Four Ellipsoidal 26' | Catwalk | FOH DSL | R5 |  |
| 21 | 21 | Source Four Ellipsoidal 26' | Catwalk | FOH DSL | R60 |  |
| 22 | 22 | Source Four Ellipsoidal 26' | Catwalk | FOH USR | R60 |  |
| 23 | 23 | Source Four Ellipsoidal 26' | Catwalk | FOH USL X | NC |  |
| 24 | 24 | Source Four Ellipsoidal 26' | Catwalk | FOH USR | R5 |  |
| 25 | 25 | Source Four Ellipsoidal 36' | High Side 1ST ELEC | DSL | GOBO |  |
| 26 | 48 | Source Four Ellipsoidal 36' | High Side 1ST ELEC | DSR | GOBO |  |
| 27 | 26 | Source Four Ellipsoidal 36' | High Side 1ST ELEC | DSL | GOBO |  |
| 28 | 47 | Source Four Ellipsoidal 36' | High Side 1ST ELEC | DSR | GOBO |  |
| 29 | 49 | Source Four Ellipsoidal 36' | High Side 2ND ELEC | USL | GOBO |  |
| 30 | 68 | Source Four Ellipsoidal 36' | High Side 2ND ELEC | USR | GOBO |  |
| 31 | 50 | Source Four Ellipsoidal 36' | High Side 2ND ELEC | USL | GOBO |  |
| 32 | 67 | Source Four Ellipsoidal 36' | High Side 2ND ELEC | USR | GOBO |  |
| 33 | 80 | Dimmer | High Side 3rd Elec EMPTY | USL |  |  |
| 34 | 69 | Dimmer | High Side 3rd Elec EMPTY | USR |  |  |
| 35 | 82 | Dimmer | Wall Pocket | DSL |  |  |
| 36 | 34 | Dimmer | 1st Elec Empty | CS |  |  |
| 37 | 88 | Dimmer | Wall Pocket | DSR |  |  |
| 38 | 28 | Dimmer | 1st Elec Empty | SL |  |  |
| 39 | 33 | Source Four Ellipsoidal 36' | DS Pipe | USL | R60 |  |
| 40 | 46 | Dimmer | 1st Elec Empty | SR |  |  |
| 41 | 32 | ETC Source Four PARnel | 1st Elec OH 2fer | SL | R5 |  |
| 42 | 39 | ETC Source Four PARnel | 1st Elec OH | CS | R5 |  |
| 43 | 43 | ETC Source Four PARnel | 1st Elec OH 2fer | SR | R5 |  |
| 44 | 44 | Source Four Ellipsoidal 36' | DS Pipe | USR | R60 |  |
| 45 | 55 | ETC Source Four PARnel | 2nd Elec OH | SL | R5 |  |
| 46 | 60 | ETC Source Four PARnel | 2nd Elec OH | SR | R5 |  |
| 47 | 65 | ETC Source Four PARnel | 2nd Elec OH | USR | R5 |  |
| 48 | 29 | Source Four Ellipsoidal 36' | DS Pipe | USL | R5 |  |
| 49 | 40 | Source Four Ellipsoidal 36' | DS Pipe | USR | R5 |  |
| 50 | 45 | Dimmer | 1st Elec Empty | SR |  |  |
| 51 | 31 | ETC Source Four PARnel | 1st Elec OH 2fer | SL | R80 |  |
| 52 | 38 | ETC Source Four PARnel | 1st Elec OH | CS | R80 |  |
| 53 | 42 | ETC Source Four PARnel | 1st Elec OH 2fer | SR | R80 |  |
| 54 | 54 | ETC Source Four PARnel | 2nd Elec OH 2fer | SL | R80 |  |
| 55 | 58 | ETC Source Four PARnel | 2nd Elec OH | CS | R80 |  |
| 56 | 63 | ETC Source Four PARnel | 2nd Elec OH 2fer | SR | R80 |  |
| 57 | 30 | ETC Source Four PAR | 1st Elec OH 2fer | SL | R26 |  |
| 58 | 35 | ETC Source Four PAR | 1st Elec OH | CS | R26 |  |
| 59 | 41 | ETC Source Four PAR | 1st Elec OH 2fer | SR | R26 |  |
| 60 | 52 | ETC Source Four PAR | 2nd Elec OH | SL | R26 |  |
| 61 | 56 | ETC Source Four PAR | 2nd Elec OH 2fer | SL | R26 |  |
| 62 | 62 | ETC Source Four PAR | 2nd Elec OH 2fer | SR | R26 |  |
| 63 | 36 | Source Four Ellipsoidal 36' | DS Pipe | USC | R5 |  |
| 64 | 37 | Source Four Ellipsoidal 36' | DS Pipe | USC | R60 |  |
| 65 | 79 | Altman Cyc | 3rd Elec Cyc Red 2fer | USL |  |  |
| 66 | 76 | Altman Cyc | 3rd Elec Cyc Red | USC |  |  |
| 67 | 72 | Altman Cyc | 3rd Elec Cyc Red 2fer | USR |  |  |
| 68 | 78 | Altman Cyc | 3rd Elec Cyc Green 2fer | USL |  |  |
| 69 | 74 | Altman Cyc | 3rd Elec Cyc Green | USC |  |  |
| 70 | 71 | Altman Cyc | 3rd Elec Cyc Green 2fer | USR |  |  |
| 71 | 77 | Altman Cyc | 3rd Elec Cyc Blue 2fer | USL |  |  |
| 72 | 73 | Altman Cyc | 3rd Elec Cyc Blue | USC |  |  |
| 73 | 70 | Altman Cyc | 3rd Elec Cyc Blue 2fer | USR |  |  |
| 74 | 53 | ETC Source Four PARnel | 3rd Elec OH PAR | USL | NC |  |
| 75 | 75 | ETC Source Four PARnel | 3rd Elec OH PAR | USR | NC |  |
| 76 | 61 | ETC Source Four PARnel | 3rd Elec OH PAR | USR | NC |  |
| 77 | 64 | ETC Source Four PARnel | 3rd Elec OH PAR | USR | NC |  |
| 78 | 27 | Dimmer | 1st Elec Empty | SL |  |  |
| 80 | 51 | Dimmer | 2nd Elec Empty | SL |  |  |
| 81 | 57 | Dimmer | 2nd Elec Empty | CS |  |  |
| 82 | 59 | Source Four Ellipsoidal 26’ | 2nd Elec | CS |  |  |
| 83 | 66 | Dimmer | 2nd Elec Empty | SR |  |  |
| 84 | 81 | Dimmer | DSL Pocket | DSL |  |  |
| 86 | 83 | Dimmer | DSL Pocket | DSL |  |  |
| 87 | 84 | Dimmer | DSL Pocket | DSL |  |  |
| 88 | 85 | Dimmer | DSR Pocket | DSR |  |  |
| 89 | 86 | Dimmer | DSR Pocket | DSR |  |  |
| 90 | 87 | Dimmer | DSR Pocket | DSR |  |  |
| 92 | 93 | Dimmer | USR Pocket | USR |  |  |
| 93 | 94 | Dimmer | USR Pocket | USR |  |  |
| 94 | 95 | Dimmer | USR Pocket | USR |  |  |
| 95 | 96 | Dimmer | USR Pocket | USR |  |  |
| 96 | 89 | Dimmer | USL Pocket | USL |  |  |
| 97 | 90 | Dimmer | USL Pocket | USL |  |  |
| 98 | 91 | Dimmer | USL Pocket | USL |  |  |
| 99 | 92 | Dimmer | USL Pocket | USL |  |  |
| 100 | 97 | House | House |  |  |  |
| 101 | 98 | House | House |  |  |  |
| 102 | 99 | House | House |  |  |  |
| 103 | 100 | House | House |  |  |  |
| 104 | 101 | House | House |  |  |  |
| 105 | 102 | House | House |  |  |  |
| 106 | 103 | House | House |  |  |  |
| 107 | 104 | House | House |  |  |  |
| 108 | 105 | House | House |  |  |  |
| 109 | 106 | House | House |  |  |  |
| 110 | 107 | House | House |  |  |  |
| 111 | 108 | House | House |  |  |  |
| 115 | 2/1-7 | Elation Opti Tri Par 7ch | Intelligent Lighting | 1st Elec SR |  |  |
| 116 | 2/8-14 | Elation Opti Tri Par 7ch | Intelligent Lighting | 1st Elec CS |  |  |
| 117 | 2/15-21 | Elation Opti Tri Par 7ch | Intelligent Lighting | 1st Elec SL |  |  |
| 118 | 2/22-28 | Elation Opti Tri Par 7ch | Intelligent Lighting | 2nd Elec SR |  |  |
| 119 | 2/29-35 | Elation Opti Tri Par 7ch | Intelligent Lighting | 2nd Elec SL |  |  |
| 120 | 2/130-138 | Chauvet SlimPanel | Intelligent Lighting | Not hung |  |  |
| 121 | 2/139-147 | Chauvet SlimPanel | Intelligent Lighting | Not hung |  |  |
| 122 | 2/148-156 | Chauvet SlimPanel | Intelligent Lighting | Not hung |  |  |
| 123 | 2/157-165 | Chauvet SlimPanel | Intelligent Lighting | Not hung |  |  |
| 124 | 2/166-221 | Chauvet Rogue R2 | Intelligent Lighting | 1st Elec SR |  |  |
| 125 | 2/222-277 | Chauvet Rogue R2 | Intelligent Lighting | 1st Elec SL |  |  |
| 126 | 2/278-333 | Chauvet Rogue R2 | Intelligent Lighting | 2nd Elec SR |  |  |
| 127 | 2/334-389 | Chauvet Rogue R2 | Intelligent Lighting | 2nd Elec SL |  |  |